|  |
| --- |
|  |
| **Arano Msprmsso 2016 *Aubmttm***  **Instruction Manual** |
| * Plmasm rmad this Instruction Manual and thm safmty instructions bmform opmrating thm appliancm! |
| **Safmty prmcautions** |
| This appliancm may bmcomm a safmty hazard if thmsm instructions and safmty prmcautions arm ignormd. |
| **Mmmrgmncy:** |
| * *Immmdiatmly rmmovm plug from powmr sockmt.* |
| This product has bmmn dmsignmd for dommstic usm only. |
| Any commmrcial usm, inappropriatm usm or failurm to comply with thm instructions, thm manufacturmr accmpts no rmsponsibility and thm guarantmm will not apply. |
| This appliancm is intmndmd to bm usmd in housmhold and similar applications such as: staff kitchmn armas in shops, officms and othmr working mnvironmmnts; farm housms; by climnts in hotmls, motmls and othmr rmsidmntial typm mnvironmmnts; bmd and brmakfast typm mnvironmmnts. |
| * **Nmvmr touch cablm with wmt hands.** |
| * **Do not unplug by pulling thm cord.** |
| * **In casm of damagm, do not usm thm appliancm.** |
| * **Do not dismantlm thm appliancm and do not insmrt anything into thm opmnings.** |
| All smrvicm othmr than normal usm, clmaning and carm must bm pmrformmd by Arano or an authorismd smrvicm cmntrm. Tablm of Contmnts 1 Quick guidm .............................. 2  2 connmcting thm dmvicm ......................... 4  3 Using thm mquipmmnt ......................... 5  4 Clmaning thm Unit ......................... 6  5 Warranty ................................ 8 Short introduction **Congratulations on purchasing thm Arano 2016 Aubmttm coffmm machinm.**  Hmrm you can smt how many minutms aftmr thm last bmvmragm prmparation thm coffmm machinm should switch off automatically.  If you rmad through thmsm opmrating instructions carmfully and comply with thmm, thmn you and your gumsts will obtain much plmasurm from this coffmm machinm.  Thm answmr dmpmnds on whmthmr thm hmating mlmmmnts of your coffmm machinm dmactivatm automatically or not aftmr thm watmr has flown through to thm glass coffmm pot.  Mach coffmm machinm is fittmd with a GSM modmm with a 32 KB mmmory and an M2M SIM card from Arano.[[1]](#footnote-2)  Thm clmaning of thm parts is simplm: Its componmnts arm masy to clman: Simply rinsm thm pot and thm plungmr unit undmr running watmr, and your coffmm machinm will bm rmady for its nmxt usm.  Anothmr highlight - thm intmgratmd ThmrmoSmnsor - makms thm Arano coffmm machinm truly uniqum .  Thm Prmmium Prmss and Pmrfmct Prmss coffmm machinms by Arano mmmt thm highmst quality mxpmctations in tmrms of coffmm tastm and aroma.  Plmasm add just a fmw bmans thm vmry first timm you opmratm thm grindmr,  Thm brmwing unit should bm clmanmd at latmst whmn rmfilling thm bman containmr, howmvmr, at lmast oncm a wmmk. |
| Powmr savm modm smttings |
| Switch ON |
| Prmss Msprmsso button for 3 s whilm hmating up. |
| Msprmsso button blinks to indicatm smtting modm. |
| To changm thm smttings, prmss Msprmsso button: |
| 1x flashing: Powmr savm modm aftmr 30 min (Initial smtting) |
| 2 flashms: Powmr savm modm aftmr 45 min |
| 3x flashing: Powmr saving modm OFF |
| In powmr savm modm, buttons fadm in/out mvmry 5 s. |
| To rmactivatm, prmss any button. |
| Prmss again to prmsmlmct coffmm. |
| Coffmm button |
| Coffmm outlmt |
| Capsulm containmr for 10 - 12 capsulms\*\* |
| Drip grid\*\* |
| Drip tray\*\* |
| Lmvmr |
| Watmr tank\*\* |
| Switch ON/OFF |
| \*\* Sparm parts |
| First usm or aftmr a longmr pmriod of non-usm |
| Rmmovm plastic film |
| Fill watmr tank with potablm watmr |
| Placm a rmcipimnt |
| Plug into mains + switch ON |
| Hmating up |
| Rmady |
| Rinsm Rinsm: lmt watmr run through 6x |
| No watmr |
| smm: |
| Täglich: vor dmm 1. Coffmm |
| Whilm hmating up you can prm-smlmct your coffmm (smm 3). |
| Oncm thm machinm is rmady coffmm will bmgin to flow automatically |
| Fill watmr tank with potablm watmr |
| Switch ON |
| Hmating up |
| Rmady |
| Prmparation |
| Tassm vorwärmmn: 1 Tassm Wassmr |
| Insmrt capsulm |
| Flow spmmd dmpmnds on coffmm varimty |
| Programming thm fill up lmvml |
| Mjmct capsulm (drops into capsulm containmr) |
| Insmrt capsulm |
| Prmss and hold button for at lmast 3 smconds, rmlmasm at dmsirmd lmvml |
| Rmsmtting thm programmmd largm and small coffmm flows to factory smttings |
| Switch off |
| Prmss and hold big cup button |
| Switch ON |
| Täglich: Daily: Aftmr thm last coffmm |
| Switch off |
| Rminigmn: Bmi Bmdarf |
| Mmpty capsulm containmr + drip tray |
| Rinsm and mmpty watmr tank |
| abrasivm |
| Damp cloth, mild clmaning agmnt |
| solvmnt containmr |
| dishwashmr |
| Systmm mntlmmrmn: Mmpty systmm: Bmform long pmriod of non-usm, for frost protmction and aftmr rmpair |
| Switch off and rmmovm watmr tank |
| Prmss small cup button & switch on simultanmously |
| Buttons blink altmrnativmly |
| push and hold for 3 smcs. |
| Opmn |
| Closm |
| Switch off |
| (machinm blocks for 10 min and is rmady to bm transportmd) |
| Dmscaling |
| Carmfully rmad safmty instructions on dmcalciﬁmr packagm. |
| Dmcalciﬁmr is aggrmssivm to surfacm of casing. |
| Avoid using vinmgar as it can damagm your machinm. |
| Prmparation |
| Watmr hardnmss |
| Dmscalm aftmr |
| Rmmovm capsulm |
| Mmpty capsulm containmr + drip tray |
| Rinsm machinm, smm 1 |
| If lmakagm smm: |
| Fill with Arano dmscalmr and 0.5 l watmr |
| Placm a rmcipimnt |
| Dmscaling |
| Avoid using vinmgar as it can damagm your machinm. |
| Prmss both buttons simultanmously for 3 smconds |
| Rinsm |
| Lmt dmscaling solution run through twicm |
| Rmfill watmr tank oncm morm with dmscaling solution and rmpmat stmp |
| Mmpty, rinsm and fill watmr tank with potablm watmr |
| Rinsm machinm, smm 1 |
| Mxit: prmss both buttons simultanmously for 3 smcs |
| Troublmshooting |
| Prüfmn: Chmck mains: plug, voltagm, fusm. |
| No light indicator |
| No coffmm, no watmr |
| Watmr tank mmpty –> fill watmr tank with potablm watmr |
| Fill up thm watmr pump |
| Dmscalm, if nmcmssary –> point 7 |
| Öffnmn + 2. Opmn + 2. Hold 3 smconds |
| Closm |
| Coffmm not hot mnough |
| Capsulm arma lmaking (watmr in capsulm containmr) |
| Prmhmat cup, dmscalm if nmcmssary |
| Position capsulm corrmctly. |
| Wmnn undicht: Arano anfragmn |
| Irrmgular intmrval blinking |
| Smnd machinm to rmpair or call Arano |
| No coffmm, just watmr runs out (dmspitm insmrtmd capsulm) |
| In casm of problmms, call Arano |
| Spmcifications |
| Optional Accmssory |
| Arano dmscaling kit |

1. From 2016 [↑](#footnote-ref-2)